(export (version D)
  (design
    (source "C:\\Users\\Magnus\\Documents\\Dream6800\\KiCad - Dream 6800\\Dream_6800.sch")
    (date "02.03.2019 16:08:16")
    (tool "Eeschema (5.0.2)-1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date "4 jan 2019")
        (source Dream_6800.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U1)
      (value MC6800)
      (footprint Package_DIP:DIP-40_W15.24mm_LongPads)
      (libsource (lib Dream_6800) (part MC6800) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C692295))
    (comp (ref U8)
      (value MC6875)
      (footprint Package_DIP:DIP-16_W7.62mm_LongPads)
      (libsource (lib Dream_6800) (part MC6875) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6922CC))
    (comp (ref X1)
      (value 4Mhz)
      (footprint Crystal:Crystal_HC33-U_Vertical)
      (datasheet ~)
      (libsource (lib Device) (part Crystal) (description "Two pin crystal"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6922D9))
    (comp (ref C11)
      (value 150pF)
      (footprint Capacitor_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6922E0))
    (comp (ref L2)
      (value 10uH)
      (footprint Inductor_THT:L_Axial_L7.0mm_D3.3mm_P12.70mm_Horizontal_Fastron_MICC)
      (datasheet ~)
      (libsource (lib Dream_6800) (part INDUCTOR_SMALL) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6922E7))
    (comp (ref R10)
      (value 1k)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6922EE))
    (comp (ref C12)
      (value 2.2uF)
      (footprint Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C692317))
    (comp (ref U15)
      (value 74LS93)
      (footprint Package_DIP:DIP-14_W7.62mm_LongPads)
      (datasheet ~)
      (libsource (lib Dream_6800) (part 74LS93) (description "Divide by 2 & 8 counter"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6A6E57))
    (comp (ref U14)
      (value 74LS93)
      (footprint Package_DIP:DIP-14_W7.62mm_LongPads)
      (datasheet ~)
      (libsource (lib Dream_6800) (part 74LS93) (description "Divide by 2 & 8 counter"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6A6E5E))
    (comp (ref U19)
      (value 74LS123)
      (footprint Package_DIP:DIP-16_W7.62mm_LongPads)
      (libsource (lib Dream_6800) (part 74LS123) (description "Dual retriggerable Monostable"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6A6E84))
    (comp (ref U16)
      (value 74LS20)
      (footprint Package_DIP:DIP-14_W7.62mm_LongPads)
      (libsource (lib Dream_6800) (part 74LS20) (description "Dual Nand 4 inputs"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6A6E93))
    (comp (ref C6)
      (value 150pF)
      (footprint Capacitor_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6A6EBC))
    (comp (ref R2)
      (value 10k)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6A6EC3))
    (comp (ref R3)
      (value 220)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6A6EDD))
    (comp (ref R4)
      (value 120)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6A6EE4))
    (comp (ref C7)
      (value 3n3)
      (footprint Capacitor_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6A6EF6))
    (comp (ref U17)
      (value 74LS04)
      (footprint Package_DIP:DIP-14_W7.62mm_LongPads)
      (libsource (lib Dream_6800) (part 74LS04) (description "Hex Inverseur"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6A6F01))
    (comp (ref U18)
      (value 74LS11)
      (footprint Package_DIP:DIP-14_W7.62mm_LongPads)
      (libsource (lib Dream_6800) (part 74LS11) (description "Triple And3"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6A6F08))
    (comp (ref U7)
      (value CD4014)
      (footprint Package_DIP:DIP-16_W7.62mm_LongPads)
      (libsource (lib Dream_6800) (part CD4014) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6A6F16))
    (comp (ref R6)
      (value 470)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6A6F3C))
    (comp (ref U13)
      (value CD4040)
      (footprint Package_DIP:DIP-16_W7.62mm_LongPads)
      (libsource (lib Dream_6800) (part CD4040) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6A6F55))
    (comp (ref C8)
      (value 100nF)
      (footprint Capacitor_THT:C_Rect_L9.0mm_W2.5mm_P7.50mm_MKT)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6A6FA9))
    (comp (ref R5)
      (value 10k)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6A6FB0))
    (comp (ref C9)
      (value 47pf)
      (footprint Capacitor_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6A6FFA))
    (comp (ref R8)
      (value 2k2)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6A7001))
    (comp (ref R7)
      (value 2k2)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6A7008))
    (comp (ref R9)
      (value 75)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6A700F))
    (comp (ref U6)
      (value 74LS367)
      (footprint Package_DIP:DIP-16_W7.62mm_LongPads)
      (datasheet ~)
      (libsource (lib 74xx) (part 74LS367) (description "Hex Bus Driver 3-state outputs"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6A7042))
    (comp (ref U5)
      (value 74LS367)
      (footprint Package_DIP:DIP-16_W7.62mm_LongPads)
      (datasheet ~)
      (libsource (lib 74xx) (part 74LS367) (description "Hex Bus Driver 3-state outputs"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6A7049))
    (comp (ref U10)
      (value 74LS10)
      (footprint Package_DIP:DIP-14_W7.62mm_LongPads)
      (libsource (lib Dream_6800) (part 74LS10) (description "Triple Nand3"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6D4B40))
    (comp (ref U11)
      (value 74LS04)
      (footprint Package_DIP:DIP-14_W7.62mm_LongPads)
      (libsource (lib Dream_6800) (part 74LS04) (description "Hex Inverseur"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6D4BBF))
    (comp (ref U20)
      (value 7440)
      (footprint Package_DIP:DIP-14_W7.62mm_LongPads)
      (libsource (lib Dream_6800) (part 74LS40) (description "Dual Nand 4 inputs"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C7C888D))
    (comp (ref R12)
      (value 2k2)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C7C88A8))
    (comp (ref R18)
      (value 2k2)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C7C88D8))
    (comp (ref R27)
      (value 47)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C7C88EC))
    (comp (ref U12)
      (value 74LS08)
      (footprint Package_DIP:DIP-14_W7.62mm_LongPads)
      (libsource (lib Dream_6800) (part 74LS08) (description "Quad And2"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C7C890D))
    (comp (ref R26)
      (value 470)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C7C891A))
    (comp (ref R31)
      (value 220)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C7C8921))
    (comp (ref R30)
      (value 2k2)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C7C8928))
    (comp (ref R23)
      (value 4k7)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C7C892F))
    (comp (ref C17)
      (value 10uF)
      (footprint Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C7C8936))
    (comp (ref U9)
      (value MC6820)
      (footprint Package_DIP:DIP-40_W15.24mm_LongPads)
      (libsource (lib Dream_6800) (part MC6820) (description "Interface parallele 2 x 8 bits"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C7C897F))
    (comp (ref U23)
      (value LM741)
      (footprint Package_DIP:DIP-8_W7.62mm_LongPads)
      (datasheet ~)
      (libsource (lib Dream_6800) (part LM741) (description "Op amp"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C85B6E7))
    (comp (ref U22)
      (value 74121)
      (footprint Package_DIP:DIP-14_W7.62mm_LongPads)
      (datasheet ~)
      (libsource (lib Dream_6800) (part 74LS121) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C85B6EE))
    (comp (ref U21)
      (value 74LS74)
      (footprint Package_DIP:DIP-14_W7.62mm_LongPads)
      (datasheet 74xx/74hc_hct74.pdf)
      (libsource (lib Dream_6800) (part 74LS74) (description "Dual D FlipFlop, Set & Reset"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C85B6F5))
    (comp (ref C15)
      (value 33nF)
      (footprint Capacitor_THT:C_Rect_L9.0mm_W2.5mm_P7.50mm_MKT)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C85B6FC))
    (comp (ref R21)
      (value 10k)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C85B70A))
    (comp (ref R28)
      (value 22k)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C85B73D))
    (comp (ref R32)
      (value 22k)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C85B744))
    (comp (ref C36)
      (value 10nF)
      (footprint Capacitor_THT:C_Rect_L9.0mm_W2.5mm_P7.50mm_MKT)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C85B74B))
    (comp (ref R14)
      (value 1k5)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C85B770))
    (comp (ref R13)
      (value 10k)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C85B777))
    (comp (ref R16)
      (value 1k5)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C85B77E))
    (comp (ref R20)
      (value 5k8)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C85B785))
    (comp (ref C13)
      (value 1nF)
      (footprint Capacitor_THT:C_Rect_L9.0mm_W2.5mm_P7.50mm_MKT)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C85B78C))
    (comp (ref C14)
      (value 22nF)
      (footprint Capacitor_THT:C_Rect_L9.0mm_W2.5mm_P7.50mm_MKT)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C85B793))
    (comp (ref R17)
      (value 10k)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C85B79A))
    (comp (ref R22)
      (value 4k7)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C85B7A1))
    (comp (ref C16)
      (value 10nF)
      (footprint Capacitor_THT:C_Rect_L9.0mm_W2.5mm_P7.50mm_MKT)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C85B7A8))
    (comp (ref R24)
      (value 6k8)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C85B7AF))
    (comp (ref R25)
      (value 2k2)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C85B7B6))
    (comp (ref R15)
      (value 1k5)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C85B7BD))
    (comp (ref U24)
      (value NE566)
      (footprint Package_DIP:DIP-8_W7.62mm_LongPads)
      (libsource (lib Dream_6800) (part NE566) (description "Function Generator"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C85B7CB))
    (comp (ref D5)
      (value BAT43)
      (footprint Diode_THT:D_DO-34_SOD68_P12.70mm_Horizontal)
      (datasheet http://www.vishay.com/docs/85660/bat42.pdf)
      (libsource (lib Diode) (part BAT43) (description "30V 0.2A Small Signal Schottky Diode, DO-35"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E31A9C3))
    (comp (ref Q2)
      (value 2N3906)
      (footprint Package_TO_SOT_THT:TO-5-3)
      (datasheet https://www.fairchildsemi.com/datasheets/2N/2N3906.pdf)
      (libsource (lib Transistor_BJT) (part 2N3906) (description "-0.2A Ic, -40V Vce, Small Signal PNP Transistor, TO-92"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EF62E1D))
    (comp (ref D2)
      (value 1N4148)
      (footprint Diode_THT:D_DO-34_SOD68_P12.70mm_Horizontal)
      (datasheet http://www.nxp.com/documents/data_sheet/1N4148_1N4448.pdf)
      (libsource (lib Diode) (part 1N4148) (description "100V 0.15A standard switching diode, DO-35"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F6C1E84))
    (comp (ref D3)
      (value 1N4148)
      (footprint Diode_THT:D_DO-34_SOD68_P12.70mm_Horizontal)
      (datasheet http://www.nxp.com/documents/data_sheet/1N4148_1N4448.pdf)
      (libsource (lib Diode) (part 1N4148) (description "100V 0.15A standard switching diode, DO-35"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F6C2243))
    (comp (ref D4)
      (value 1N4148)
      (footprint Diode_THT:D_DO-34_SOD68_P12.70mm_Horizontal)
      (datasheet http://www.nxp.com/documents/data_sheet/1N4148_1N4448.pdf)
      (libsource (lib Diode) (part 1N4148) (description "100V 0.15A standard switching diode, DO-35"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F6C2C3D))
    (comp (ref Q1)
      (value 2N3904)
      (footprint Package_TO_SOT_THT:TO-5-3)
      (datasheet https://www.fairchildsemi.com/datasheets/2N/2N3904.pdf)
      (libsource (lib Transistor_BJT) (part 2N3904) (description "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F6C30F5))
    (comp (ref J1)
      (value Conn_Coaxial)
      (footprint TerminalBlock:TerminalBlock_bornier-2_P5.08mm)
      (datasheet " ~")
      (libsource (lib Connector) (part Conn_Coaxial) (description "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F6C3CD9))
    (comp (ref D1)
      (value 1N4148)
      (footprint Diode_THT:D_DO-34_SOD68_P12.70mm_Horizontal)
      (datasheet http://www.nxp.com/documents/data_sheet/1N4148_1N4448.pdf)
      (libsource (lib Diode) (part 1N4148) (description "100V 0.15A standard switching diode, DO-35"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F7FADC8))
    (comp (ref U2)
      (value 2716)
      (footprint Package_DIP:DIP-24_W15.24mm_LongPads)
      (libsource (lib Dream_6800) (part 2716) (description "SRAM 2KO"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60ADE81C))
    (comp (ref U3)
      (value 2114)
      (footprint Package_DIP:DIP-18_W7.62mm_LongPads)
      (libsource (lib Dream_6800) (part 2114) (description "SRAM 2KO"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61D44439))
    (comp (ref U4)
      (value 2114)
      (footprint Package_DIP:DIP-18_W7.62mm_LongPads)
      (libsource (lib Dream_6800) (part 2114) (description "SRAM 2KO"))
      (sheetpath (names /) (tstamps /))
      (tstamp 620429F7))
    (comp (ref J2)
      (value ExptendedKeyboard)
      (footprint Package_DIP:DIP-16_W7.62mm_LongPads)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x08_Counter_Clockwise) (description "Generic connector, double row, 02x08, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 63FDF9E7))
    (comp (ref RV1)
      (value R_POT)
      (footprint Potentiometer_THT:Potentiometer_Piher_PT-10-H01_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R_POT) (description Potentiometer))
      (sheetpath (names /) (tstamps /))
      (tstamp 648D8826))
    (comp (ref J4)
      (value ExpansionBusAdress)
      (footprint Package_DIP:DIP-16_W7.62mm_LongPads)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x08_Counter_Clockwise) (description "Generic connector, double row, 02x08, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6F4901))
    (comp (ref J5)
      (value ExpansionBusData)
      (footprint Package_DIP:DIP-16_W7.62mm_LongPads)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x08_Counter_Clockwise) (description "Generic connector, double row, 02x08, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C813B0E))
    (comp (ref J3)
      (value ExtendedI/O)
      (footprint Package_DIP:DIP-16_W7.62mm_LongPads)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x08_Counter_Clockwise) (description "Generic connector, double row, 02x08, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C813C40))
    (comp (ref J6)
      (value Conn_01x04)
      (footprint TerminalBlock:TerminalBlock_bornier-4_P5.08mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x04) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C72057E))
    (comp (ref C2)
      (value 10uF)
      (footprint Capacitor_THT:CP_Axial_L11.0mm_D5.0mm_P18.00mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CA28FA3))
    (comp (ref C4)
      (value 10uF)
      (footprint Capacitor_THT:CP_Axial_L11.0mm_D5.0mm_P18.00mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CA29BAF))
    (comp (ref C5)
      (value 100nF)
      (footprint Capacitor_THT:C_Rect_L9.0mm_W2.5mm_P7.50mm_MKT)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CA2BD12))
    (comp (ref C10)
      (value 100nF)
      (footprint Capacitor_THT:C_Rect_L9.0mm_W2.5mm_P7.50mm_MKT)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CAADF60))
    (comp (ref C18)
      (value 100nF)
      (footprint Capacitor_THT:C_Rect_L9.0mm_W2.5mm_P7.50mm_MKT)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CAAE044))
    (comp (ref C3)
      (value 100nF)
      (footprint Capacitor_THT:C_Rect_L9.0mm_W2.5mm_P7.50mm_MKT)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CAAE672))
    (comp (ref C1)
      (value 100nF)
      (footprint Capacitor_THT:C_Rect_L9.0mm_W2.5mm_P7.50mm_MKT)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CAAE902))
    (comp (ref RV2)
      (value R_POT)
      (footprint Potentiometer_THT:Potentiometer_Piher_PT-15-H05_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R_POT) (description Potentiometer))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C728037))
    (comp (ref C19)
      (value 100nF)
      (footprint Capacitor_THT:C_Axial_L3.8mm_D2.6mm_P12.50mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CD360AE))
    (comp (ref C20)
      (value 100nF)
      (footprint Capacitor_THT:C_Axial_L3.8mm_D2.6mm_P12.50mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE5371E))
    (comp (ref C21)
      (value 100nF)
      (footprint Capacitor_THT:C_Rect_L9.0mm_W2.5mm_P7.50mm_MKT)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CEE33D2))
    (comp (ref C22)
      (value 100nF)
      (footprint Capacitor_THT:C_Rect_L9.0mm_W2.5mm_P7.50mm_MKT)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CEE33D9))
    (comp (ref C23)
      (value 100nF)
      (footprint Capacitor_THT:C_Rect_L9.0mm_W2.5mm_P7.50mm_MKT)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D6E2505))
    (comp (ref C24)
      (value 100nF)
      (footprint Capacitor_THT:C_Rect_L9.0mm_W2.5mm_P7.50mm_MKT)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D6E250C))
    (comp (ref C25)
      (value 100nF)
      (footprint Capacitor_THT:C_Rect_L9.0mm_W2.5mm_P7.50mm_MKT)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C871FCC))
    (comp (ref J7)
      (value Conn_01x02)
      (footprint TerminalBlock:TerminalBlock_bornier-2_P5.08mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x02) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8DCC6C))
    (comp (ref J8)
      (value Conn_01x02)
      (footprint Connector_Wire:SolderWirePad_1x02_P3.81mm_Drill1mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x02) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CACA56A)))
  (libparts
    (libpart (lib 74xx) (part 74LS367)
      (description "Hex Bus Driver 3-state outputs")
      (docs http://www.ti.com/lit/gpn/sn74LS367)
      (footprints
        (fp DIP?16*))
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS367))
      (pins
        (pin (num 1) (name OEa) (type input))
        (pin (num 2) (name I1) (type input))
        (pin (num 3) (name O1a) (type 3state))
        (pin (num 4) (name I2) (type input))
        (pin (num 5) (name O2a) (type 3state))
        (pin (num 6) (name I3) (type input))
        (pin (num 7) (name O3a) (type 3state))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name O4a) (type 3state))
        (pin (num 10) (name I4) (type input))
        (pin (num 11) (name O5b) (type 3state))
        (pin (num 12) (name I5) (type input))
        (pin (num 13) (name O6b) (type 3state))
        (pin (num 14) (name I6) (type input))
        (pin (num 15) (name OEb) (type input))
        (pin (num 16) (name VCC) (type power_in))))
    (libpart (lib Connector) (part Conn_Coaxial)
      (description "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)")
      (docs " ~")
      (footprints
        (fp *BNC*)
        (fp *SMA*)
        (fp *SMB*)
        (fp *SMC*)
        (fp *Cinch*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_Coaxial))
      (pins
        (pin (num 1) (name In) (type passive))
        (pin (num 2) (name Ext) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x02)
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x04)
      (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x04))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x08_Counter_Clockwise)
      (description "Generic connector, double row, 02x08, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x08_Counter_Clockwise))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part CP)
      (description "Polarized capacitor")
      (docs ~)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part Crystal)
      (description "Two pin crystal")
      (docs ~)
      (footprints
        (fp Crystal*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part R_POT)
      (description Potentiometer)
      (docs ~)
      (footprints
        (fp Potentiometer*))
      (fields
        (field (name Reference) RV)
        (field (name Value) R_POT))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib Diode) (part 1N4148)
      (aliases
        (alias 1N4448)
        (alias 1N4149)
        (alias 1N4151)
        (alias 1N914)
        (alias BA243)
        (alias BA244)
        (alias BA282)
        (alias BA283)
        (alias BAV17)
        (alias BAV18)
        (alias BAV19)
        (alias BAV20)
        (alias BAV21)
        (alias BAW75)
        (alias BAW76)
        (alias BAY93))
      (description "100V 0.15A standard switching diode, DO-35")
      (docs http://www.nxp.com/documents/data_sheet/1N4148_1N4448.pdf)
      (footprints
        (fp D*DO?35*))
      (fields
        (field (name Reference) D)
        (field (name Value) 1N4148)
        (field (name Footprint) Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Diode) (part 1N6263)
      (aliases
        (alias BAT41)
        (alias BAT42)
        (alias BAT43)
        (alias BAT46)
        (alias BAT48RL)
        (alias BAT85)
        (alias BAT86S)
        (alias BAT86)
        (alias 1N5711)
        (alias 1N5712)
        (alias 1N6857)
        (alias 1N6858)
        (alias DSB5712)
        (alias DSB2810))
      (description "60V 15mA Schottky diode, DO-35")
      (docs www.st.com/resource/en/datasheet/1n6263.pdf)
      (footprints
        (fp D*DO?35*))
      (fields
        (field (name Reference) D)
        (field (name Value) 1N6263)
        (field (name Footprint) Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Dream_6800) (part 2114)
      (description "SRAM 2KO")
      (fields
        (field (name Reference) U)
        (field (name Value) 2114))
      (pins
        (pin (num 1) (name A6) (type input))
        (pin (num 2) (name A5) (type input))
        (pin (num 3) (name A4) (type input))
        (pin (num 4) (name A3) (type input))
        (pin (num 5) (name A0) (type input))
        (pin (num 6) (name A1) (type input))
        (pin (num 7) (name A2) (type input))
        (pin (num 8) (name ~E) (type input))
        (pin (num 9) (name GND) (type power_in))
        (pin (num 10) (name ~WR) (type input))
        (pin (num 11) (name Q3) (type 3state))
        (pin (num 12) (name Q2) (type 3state))
        (pin (num 13) (name Q1) (type 3state))
        (pin (num 14) (name Q0) (type 3state))
        (pin (num 15) (name A9) (type input))
        (pin (num 16) (name A8) (type input))
        (pin (num 17) (name A7) (type input))
        (pin (num 18) (name Vcc) (type power_in))))
    (libpart (lib Dream_6800) (part 2716)
      (description "SRAM 2KO")
      (fields
        (field (name Reference) U)
        (field (name Value) 2716))
      (pins
        (pin (num 1) (name A7) (type input))
        (pin (num 2) (name A6) (type input))
        (pin (num 3) (name A5) (type input))
        (pin (num 4) (name A4) (type input))
        (pin (num 5) (name A3) (type input))
        (pin (num 6) (name A2) (type input))
        (pin (num 7) (name A1) (type input))
        (pin (num 8) (name A0) (type input))
        (pin (num 9) (name Q0) (type 3state))
        (pin (num 10) (name Q1) (type 3state))
        (pin (num 11) (name Q2) (type 3state))
        (pin (num 12) (name GND) (type power_in))
        (pin (num 13) (name Q3) (type 3state))
        (pin (num 14) (name Q4) (type 3state))
        (pin (num 15) (name Q5) (type 3state))
        (pin (num 16) (name Q6) (type 3state))
        (pin (num 17) (name Q7) (type 3state))
        (pin (num 18) (name E) (type input))
        (pin (num 19) (name A10) (type input))
        (pin (num 20) (name G) (type input))
        (pin (num 21) (name ~WR) (type input))
        (pin (num 22) (name A9) (type input))
        (pin (num 23) (name A8) (type input))
        (pin (num 24) (name Vcc) (type power_in))))
    (libpart (lib Dream_6800) (part 74LS04)
      (description "Hex Inverseur")
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS04))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type output))
        (pin (num 3) (name ~) (type input))
        (pin (num 4) (name ~) (type output))
        (pin (num 5) (name ~) (type input))
        (pin (num 6) (name ~) (type output))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name ~) (type output))
        (pin (num 9) (name ~) (type input))
        (pin (num 10) (name ~) (type output))
        (pin (num 11) (name ~) (type input))
        (pin (num 12) (name ~) (type output))
        (pin (num 13) (name ~) (type input))
        (pin (num 14) (name VCC) (type power_in))))
    (libpart (lib Dream_6800) (part 74LS08)
      (aliases
        (alias 74LS09))
      (description "Quad And2")
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS08))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type input))
        (pin (num 3) (name ~) (type output))
        (pin (num 4) (name ~) (type input))
        (pin (num 5) (name ~) (type input))
        (pin (num 6) (name ~) (type output))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name ~) (type output))
        (pin (num 9) (name ~) (type input))
        (pin (num 10) (name ~) (type input))
        (pin (num 11) (name ~) (type output))
        (pin (num 12) (name ~) (type input))
        (pin (num 13) (name ~) (type input))
        (pin (num 14) (name VCC) (type power_in))))
    (libpart (lib Dream_6800) (part 74LS10)
      (description "Triple Nand3")
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS10))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type input))
        (pin (num 3) (name ~) (type input))
        (pin (num 4) (name ~) (type input))
        (pin (num 5) (name ~) (type input))
        (pin (num 6) (name ~) (type output))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name ~) (type output))
        (pin (num 9) (name ~) (type input))
        (pin (num 10) (name ~) (type input))
        (pin (num 11) (name ~) (type input))
        (pin (num 12) (name ~) (type output))
        (pin (num 13) (name ~) (type input))
        (pin (num 14) (name VCC) (type power_in))))
    (libpart (lib Dream_6800) (part 74LS11)
      (description "Triple And3")
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS11))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type input))
        (pin (num 3) (name ~) (type input))
        (pin (num 4) (name ~) (type input))
        (pin (num 5) (name ~) (type input))
        (pin (num 6) (name ~) (type output))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name ~) (type output))
        (pin (num 9) (name ~) (type input))
        (pin (num 10) (name ~) (type input))
        (pin (num 11) (name ~) (type input))
        (pin (num 12) (name ~) (type output))
        (pin (num 13) (name ~) (type input))
        (pin (num 14) (name VCC) (type power_in))))
    (libpart (lib Dream_6800) (part 74LS121)
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS121))
      (pins
        (pin (num 1) (name ~Q) (type output))
        (pin (num 3) (name A1) (type input))
        (pin (num 4) (name A2) (type input))
        (pin (num 5) (name B) (type input))
        (pin (num 6) (name Q) (type output))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 9) (name Rint) (type input))
        (pin (num 10) (name Cx) (type input))
        (pin (num 11) (name Rx) (type input))
        (pin (num 14) (name VCC) (type power_in))))
    (libpart (lib Dream_6800) (part 74LS123)
      (description "Dual retriggerable Monostable")
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS123))
      (pins
        (pin (num 1) (name ~A) (type input))
        (pin (num 2) (name B) (type input))
        (pin (num 3) (name ~Clr) (type input))
        (pin (num 4) (name ~Q) (type output))
        (pin (num 5) (name Q) (type output))
        (pin (num 6) (name Cx) (type input))
        (pin (num 7) (name Rx) (type input))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name ~A) (type input))
        (pin (num 10) (name B) (type input))
        (pin (num 11) (name ~Clr) (type input))
        (pin (num 12) (name ~Q) (type output))
        (pin (num 13) (name Q) (type output))
        (pin (num 14) (name Cx) (type input))
        (pin (num 15) (name Rx) (type input))
        (pin (num 16) (name VCC) (type power_in))))
    (libpart (lib Dream_6800) (part 74LS20)
      (aliases
        (alias 74LS22)
        (alias 74LS40))
      (description "Dual Nand 4 inputs")
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS20))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type input))
        (pin (num 3) (name NC) (type unspc))
        (pin (num 3-UB) (name NC) (type unspc))
        (pin (num 4) (name ~) (type input))
        (pin (num 5) (name ~) (type input))
        (pin (num 6) (name ~) (type output))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name ~) (type output))
        (pin (num 9) (name ~) (type input))
        (pin (num 10) (name ~) (type input))
        (pin (num 11) (name NC) (type unspc))
        (pin (num 11-UB) (name NC) (type unspc))
        (pin (num 12) (name ~) (type input))
        (pin (num 13) (name ~) (type input))
        (pin (num 14) (name VCC) (type power_in))))
    (libpart (lib Dream_6800) (part 74LS74)
      (aliases
        (alias 74HC74))
      (description "Dual D FlipFlop, Set & Reset")
      (docs 74xx/74hc_hct74.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS74))
      (pins
        (pin (num 1) (name Cd) (type input))
        (pin (num 2) (name D) (type input))
        (pin (num 3) (name Cp) (type input))
        (pin (num 4) (name Sd) (type input))
        (pin (num 5) (name Q) (type output))
        (pin (num 6) (name ~Q) (type output))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name ~Q) (type output))
        (pin (num 9) (name Q) (type output))
        (pin (num 10) (name Sd) (type input))
        (pin (num 11) (name Cp) (type input))
        (pin (num 12) (name D) (type input))
        (pin (num 13) (name Cd) (type input))
        (pin (num 14) (name VCC) (type power_in))))
    (libpart (lib Dream_6800) (part 74LS93)
      (description "Divide by 2 & 8 counter")
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS93))
      (pins
        (pin (num 1) (name CP1) (type input))
        (pin (num 2) (name MR1) (type input))
        (pin (num 3) (name MR2) (type input))
        (pin (num 5) (name VCC) (type power_in))
        (pin (num 8) (name Q2) (type output))
        (pin (num 9) (name Q1) (type output))
        (pin (num 10) (name GND) (type power_in))
        (pin (num 11) (name Q3) (type output))
        (pin (num 12) (name Q0) (type output))
        (pin (num 14) (name CP0) (type input))))
    (libpart (lib Dream_6800) (part CD4014)
      (fields
        (field (name Reference) U)
        (field (name Value) CD4014))
      (pins
        (pin (num 1) (name P8) (type input))
        (pin (num 2) (name Q6) (type NotConnected))
        (pin (num 3) (name Sout) (type output))
        (pin (num 4) (name P4) (type input))
        (pin (num 5) (name P3) (type input))
        (pin (num 6) (name P2) (type input))
        (pin (num 7) (name P1) (type input))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name Load) (type input))
        (pin (num 10) (name Clk) (type input))
        (pin (num 12) (name Q7) (type NotConnected))
        (pin (num 13) (name P5) (type input))
        (pin (num 14) (name P6) (type input))
        (pin (num 15) (name P7) (type input))
        (pin (num 16) (name VCC) (type power_in))))
    (libpart (lib Dream_6800) (part CD4040)
      (fields
        (field (name Reference) U)
        (field (name Value) CD4040))
      (pins
        (pin (num 1) (name Q12) (type NotConnected))
        (pin (num 2) (name Q6) (type output))
        (pin (num 3) (name Q5) (type output))
        (pin (num 4) (name Q7) (type output))
        (pin (num 5) (name Q4) (type output))
        (pin (num 6) (name Q3) (type output))
        (pin (num 7) (name Q2) (type NotConnected))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name Q1) (type NotConnected))
        (pin (num 10) (name Clk) (type input))
        (pin (num 11) (name Reset) (type input))
        (pin (num 12) (name Q9) (type output))
        (pin (num 13) (name Q8) (type output))
        (pin (num 14) (name Q10) (type NotConnected))
        (pin (num 15) (name Q11) (type NotConnected))
        (pin (num 16) (name VCC) (type power_in))))
    (libpart (lib Dream_6800) (part INDUCTOR_SMALL)
      (fields
        (field (name Reference) L)
        (field (name Value) INDUCTOR_SMALL))
      (pins
        (pin (num 1) (name 1) (type input))
        (pin (num 2) (name 2) (type input))))
    (libpart (lib Dream_6800) (part LM741)
      (description "Op amp")
      (docs AmpliOp.sch)
      (fields
        (field (name Reference) U)
        (field (name Value) LM741))
      (pins
        (pin (num 1) (name ~) (type NotConnected))
        (pin (num 2) (name -) (type input))
        (pin (num 3) (name +) (type input))
        (pin (num 4) (name V-) (type input))
        (pin (num 5) (name ~) (type NotConnected))
        (pin (num 6) (name ~) (type output))
        (pin (num 7) (name V+) (type input))))
    (libpart (lib Dream_6800) (part MC6800)
      (fields
        (field (name Reference) U)
        (field (name Value) MC6800))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name ~HALT) (type input))
        (pin (num 3) (name 01) (type input))
        (pin (num 4) (name ~IRQ) (type input))
        (pin (num 5) (name VMA) (type output))
        (pin (num 6) (name ~NMI) (type input))
        (pin (num 7) (name BA) (type output))
        (pin (num 8) (name VCC) (type power_in))
        (pin (num 9) (name A0) (type 3state))
        (pin (num 10) (name A1) (type 3state))
        (pin (num 11) (name A2) (type 3state))
        (pin (num 12) (name A3) (type 3state))
        (pin (num 13) (name A4) (type 3state))
        (pin (num 14) (name A5) (type 3state))
        (pin (num 15) (name A6) (type 3state))
        (pin (num 16) (name A7) (type 3state))
        (pin (num 17) (name A8) (type 3state))
        (pin (num 18) (name A9) (type 3state))
        (pin (num 19) (name A10) (type 3state))
        (pin (num 20) (name A11) (type 3state))
        (pin (num 21) (name GND) (type power_in))
        (pin (num 22) (name A12) (type 3state))
        (pin (num 23) (name A13) (type 3state))
        (pin (num 24) (name A14) (type 3state))
        (pin (num 25) (name A15) (type 3state))
        (pin (num 26) (name D7) (type BiDi))
        (pin (num 27) (name D6) (type BiDi))
        (pin (num 28) (name D5) (type BiDi))
        (pin (num 29) (name D4) (type BiDi))
        (pin (num 30) (name D3) (type BiDi))
        (pin (num 31) (name D2) (type BiDi))
        (pin (num 32) (name D1) (type BiDi))
        (pin (num 33) (name D0) (type BiDi))
        (pin (num 34) (name R/~W) (type output))
        (pin (num 35) (name NC) (type passive))
        (pin (num 36) (name DBE) (type input))
        (pin (num 37) (name 02) (type input))
        (pin (num 38) (name NC) (type passive))
        (pin (num 39) (name TSC) (type input))
        (pin (num 40) (name ~RESET) (type input))))
    (libpart (lib Dream_6800) (part MC6820)
      (description "Interface parallele 2 x 8 bits")
      (fields
        (field (name Reference) U)
        (field (name Value) MC6820))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name PA0) (type input))
        (pin (num 3) (name PA1) (type input))
        (pin (num 4) (name PA2) (type input))
        (pin (num 5) (name PA3) (type input))
        (pin (num 6) (name PA4) (type input))
        (pin (num 7) (name PA5) (type input))
        (pin (num 8) (name PA6) (type input))
        (pin (num 9) (name PA7) (type input))
        (pin (num 10) (name PB0) (type input))
        (pin (num 11) (name PB1) (type input))
        (pin (num 12) (name PB2) (type input))
        (pin (num 13) (name PB3) (type input))
        (pin (num 14) (name PB4) (type input))
        (pin (num 15) (name PB5) (type input))
        (pin (num 16) (name PB6) (type input))
        (pin (num 17) (name PB7) (type input))
        (pin (num 18) (name CB1) (type input))
        (pin (num 19) (name CB2) (type input))
        (pin (num 20) (name VCC) (type power_in))
        (pin (num 21) (name R/~W) (type input))
        (pin (num 22) (name CS0) (type input))
        (pin (num 23) (name ~CS2) (type input))
        (pin (num 24) (name CS1) (type input))
        (pin (num 25) (name ENABLE) (type input))
        (pin (num 26) (name D7) (type input))
        (pin (num 27) (name D6) (type input))
        (pin (num 28) (name D5) (type input))
        (pin (num 29) (name D4) (type input))
        (pin (num 30) (name D3) (type input))
        (pin (num 31) (name D2) (type input))
        (pin (num 32) (name D1) (type input))
        (pin (num 33) (name D0) (type input))
        (pin (num 34) (name ~RESET) (type input))
        (pin (num 35) (name RS1) (type input))
        (pin (num 36) (name RS0) (type input))
        (pin (num 37) (name ~IRQB) (type openCol))
        (pin (num 38) (name ~IRQA) (type openCol))
        (pin (num 39) (name CA2) (type input))
        (pin (num 40) (name CA1) (type input))))
    (libpart (lib Dream_6800) (part MC6875)
      (fields
        (field (name Reference) U)
        (field (name Value) MC6875))
      (pins
        (pin (num 1) (name X1) (type passive))
        (pin (num 2) (name X2) (type passive))
        (pin (num 3) (name Ext_In) (type input))
        (pin (num 4) (name 4xfo) (type output))
        (pin (num 5) (name 2xfo) (type output))
        (pin (num 6) (name MR) (type input))
        (pin (num 7) (name Bus02) (type output))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name MEMclk) (type output))
        (pin (num 10) (name ~DMRQ) (type input))
        (pin (num 11) (name DMGNT) (type output))
        (pin (num 12) (name ~PO-R) (type input))
        (pin (num 13) (name 02) (type output))
        (pin (num 14) (name ~RST) (type output))
        (pin (num 15) (name 01) (type output))
        (pin (num 16) (name VCC) (type power_in))))
    (libpart (lib Dream_6800) (part NE566)
      (description "Function Generator")
      (fields
        (field (name Reference) U)
        (field (name Value) NE566))
      (pins
        (pin (num 1) (name VSS) (type power_in))
        (pin (num 3) (name Squ) (type output))
        (pin (num 4) (name Tri) (type output))
        (pin (num 5) (name Mod) (type input))
        (pin (num 6) (name R1) (type passive))
        (pin (num 7) (name C1) (type passive))
        (pin (num 8) (name VCC) (type power_in))))
    (libpart (lib Transistor_BJT) (part 2N3904)
      (description "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92")
      (docs https://www.fairchildsemi.com/datasheets/2N/2N3904.pdf)
      (footprints
        (fp TO?92*))
      (fields
        (field (name Reference) Q)
        (field (name Value) 2N3904)
        (field (name Footprint) Package_TO_SOT_THT:TO-92_Inline))
      (pins
        (pin (num 1) (name E) (type passive))
        (pin (num 2) (name B) (type passive))
        (pin (num 3) (name C) (type passive))))
    (libpart (lib Transistor_BJT) (part 2N3906)
      (aliases
        (alias 2N3905))
      (description "-0.2A Ic, -40V Vce, Small Signal PNP Transistor, TO-92")
      (docs https://www.fairchildsemi.com/datasheets/2N/2N3906.pdf)
      (footprints
        (fp TO?92*))
      (fields
        (field (name Reference) Q)
        (field (name Value) 2N3906)
        (field (name Footprint) Package_TO_SOT_THT:TO-92_Inline))
      (pins
        (pin (num 1) (name E) (type passive))
        (pin (num 2) (name B) (type input))
        (pin (num 3) (name C) (type passive)))))
  (libraries
    (library (logical 74xx)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/74xx.lib"))
    (library (logical Connector)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Connector.lib"))
    (library (logical Connector_Generic)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Connector_Generic.lib"))
    (library (logical Device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Device.lib"))
    (library (logical Diode)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Diode.lib"))
    (library (logical Dream_6800)
      (uri "C:\\Users\\Magnus\\Documents\\Dream6800\\KiCad - Dream 6800/Dream_6800.lib"))
    (library (logical Transistor_BJT)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Transistor_BJT.lib")))
  (nets
    (net (code 1) (name -5V)
      (node (ref U23) (pin 4))
      (node (ref R22) (pin 1))
      (node (ref J6) (pin 4))
      (node (ref R17) (pin 1))
      (node (ref C14) (pin 1))
      (node (ref U24) (pin 1))
      (node (ref U2) (pin 21))
      (node (ref C3) (pin 1))
      (node (ref C2) (pin 2)))
    (net (code 2) (name GND)
      (node (ref U16) (pin 7))
      (node (ref U16) (pin 7))
      (node (ref U12) (pin 7))
      (node (ref C23) (pin 2))
      (node (ref U11) (pin 7))
      (node (ref U21) (pin 7))
      (node (ref C19) (pin 2))
      (node (ref C24) (pin 2))
      (node (ref J5) (pin 5))
      (node (ref C10) (pin 2))
      (node (ref U11) (pin 7))
      (node (ref U22) (pin 7))
      (node (ref U9) (pin 1))
      (node (ref U18) (pin 7))
      (node (ref U20) (pin 7))
      (node (ref U21) (pin 7))
      (node (ref U10) (pin 7))
      (node (ref U11) (pin 7))
      (node (ref U10) (pin 7))
      (node (ref U20) (pin 7))
      (node (ref U7) (pin 8))
      (node (ref R25) (pin 2))
      (node (ref J2) (pin 12))
      (node (ref J2) (pin 13))
      (node (ref J5) (pin 12))
      (node (ref C17) (pin 2))
      (node (ref U18) (pin 7))
      (node (ref U2) (pin 18))
      (node (ref U2) (pin 12))
      (node (ref J6) (pin 2))
      (node (ref U5) (pin 8))
      (node (ref U5) (pin 2))
      (node (ref C22) (pin 2))
      (node (ref J1) (pin 2))
      (node (ref U17) (pin 7))
      (node (ref C5) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref C2) (pin 1))
      (node (ref C1) (pin 2))
      (node (ref C18) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref U17) (pin 7))
      (node (ref C20) (pin 2))
      (node (ref R28) (pin 1))
      (node (ref R32) (pin 1))
      (node (ref U22) (pin 3))
      (node (ref U22) (pin 4))
      (node (ref C21) (pin 2))
      (node (ref U6) (pin 8))
      (node (ref C7) (pin 1))
      (node (ref C12) (pin 2))
      (node (ref U12) (pin 7))
      (node (ref U1) (pin 21))
      (node (ref C25) (pin 2))
      (node (ref U17) (pin 7))
      (node (ref U1) (pin 39))
      (node (ref U1) (pin 38))
      (node (ref U19) (pin 8))
      (node (ref U15) (pin 10))
      (node (ref U14) (pin 2))
      (node (ref U15) (pin 2))
      (node (ref U14) (pin 10))
      (node (ref U15) (pin 3))
      (node (ref U3) (pin 9))
      (node (ref U17) (pin 7))
      (node (ref U14) (pin 3))
      (node (ref R9) (pin 1))
      (node (ref U1) (pin 35))
      (node (ref R8) (pin 1))
      (node (ref U11) (pin 7))
      (node (ref U10) (pin 7))
      (node (ref U19) (pin 8))
      (node (ref C9) (pin 1))
      (node (ref J7) (pin 2))
      (node (ref U11) (pin 7))
      (node (ref U1) (pin 1))
      (node (ref U4) (pin 9))
      (node (ref U17) (pin 7))
      (node (ref U13) (pin 8))
      (node (ref U12) (pin 7))
      (node (ref U18) (pin 7))
      (node (ref U19) (pin 9))
      (node (ref U8) (pin 3))
      (node (ref U17) (pin 7))
      (node (ref U11) (pin 7))
      (node (ref U8) (pin 8))
      (node (ref X1) (pin 1)))
    (net (code 3) (name VCC)
      (node (ref U19) (pin 11))
      (node (ref U1) (pin 6))
      (node (ref U1) (pin 8))
      (node (ref U8) (pin 16))
      (node (ref U14) (pin 5))
      (node (ref C18) (pin 1))
      (node (ref Q2) (pin 3))
      (node (ref C21) (pin 1))
      (node (ref U13) (pin 16))
      (node (ref C22) (pin 1))
      (node (ref U8) (pin 10))
      (node (ref U17) (pin 14))
      (node (ref U18) (pin 14))
      (node (ref U19) (pin 16))
      (node (ref U17) (pin 14))
      (node (ref U8) (pin 6))
      (node (ref RV2) (pin 2))
      (node (ref U18) (pin 14))
      (node (ref R5) (pin 2))
      (node (ref J7) (pin 1))
      (node (ref U21) (pin 10))
      (node (ref U21) (pin 13))
      (node (ref U23) (pin 7))
      (node (ref U9) (pin 20))
      (node (ref RV2) (pin 3))
      (node (ref R12) (pin 1))
      (node (ref U20) (pin 14))
      (node (ref R18) (pin 2))
      (node (ref U11) (pin 14))
      (node (ref U10) (pin 14))
      (node (ref U10) (pin 14))
      (node (ref U20) (pin 14))
      (node (ref C23) (pin 1))
      (node (ref C24) (pin 1))
      (node (ref C19) (pin 1))
      (node (ref U19) (pin 16))
      (node (ref U15) (pin 5))
      (node (ref C20) (pin 1))
      (node (ref U21) (pin 14))
      (node (ref C25) (pin 1))
      (node (ref U12) (pin 14))
      (node (ref U10) (pin 14))
      (node (ref U7) (pin 16))
      (node (ref U17) (pin 14))
      (node (ref U6) (pin 16))
      (node (ref U19) (pin 2))
      (node (ref U19) (pin 3))
      (node (ref U24) (pin 8))
      (node (ref U16) (pin 14))
      (node (ref R13) (pin 2))
      (node (ref J2) (pin 11))
      (node (ref U11) (pin 14))
      (node (ref U17) (pin 14))
      (node (ref U17) (pin 14))
      (node (ref U11) (pin 14))
      (node (ref U11) (pin 14))
      (node (ref C10) (pin 1))
      (node (ref U3) (pin 18))
      (node (ref R16) (pin 2))
      (node (ref U18) (pin 14))
      (node (ref R7) (pin 2))
      (node (ref U16) (pin 14))
      (node (ref U17) (pin 14))
      (node (ref RV1) (pin 3))
      (node (ref RV1) (pin 2))
      (node (ref R20) (pin 2))
      (node (ref U11) (pin 14))
      (node (ref U2) (pin 24))
      (node (ref R30) (pin 2))
      (node (ref U11) (pin 14))
      (node (ref J6) (pin 1))
      (node (ref U5) (pin 16))
      (node (ref Q1) (pin 3))
      (node (ref U5) (pin 14))
      (node (ref U12) (pin 14))
      (node (ref C5) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref U12) (pin 14))
      (node (ref U4) (pin 18))
      (node (ref U21) (pin 14))
      (node (ref U22) (pin 14))
      (node (ref R2) (pin 1)))
    (net (code 4) (name "Net-(U10-Pad13)")
      (node (ref U10) (pin 13))
      (node (ref U11) (pin 8)))
    (net (code 5) (name "Net-(U10-Pad6)")
      (node (ref U10) (pin 6))
      (node (ref U12) (pin 13))
      (node (ref U11) (pin 9)))
    (net (code 6) (name /RAMCS*)
      (node (ref U12) (pin 11))
      (node (ref U3) (pin 8))
      (node (ref U4) (pin 8)))
    (net (code 7) (name /ROMCS*)
      (node (ref U10) (pin 8))
      (node (ref U2) (pin 20)))
    (net (code 8) (name +12v)
      (node (ref C1) (pin 1))
      (node (ref J6) (pin 3))
      (node (ref U2) (pin 19)))
    (net (code 9) (name "Net-(C8-Pad2)")
      (node (ref C8) (pin 2))
      (node (ref U19) (pin 6)))
    (net (code 10) (name "Net-(R27-Pad1)")
      (node (ref R27) (pin 1))
      (node (ref U20) (pin 8)))
    (net (code 11) (name "Net-(C17-Pad1)")
      (node (ref R26) (pin 2))
      (node (ref R31) (pin 1))
      (node (ref R30) (pin 1))
      (node (ref C17) (pin 1)))
    (net (code 12) (name /TAPEIN)
      (node (ref J2) (pin 15))
      (node (ref C36) (pin 2)))
    (net (code 13) (name "Net-(U6-Pad3)")
      (node (ref U6) (pin 3)))
    (net (code 14) (name "Net-(U6-Pad2)")
      (node (ref U6) (pin 2)))
    (net (code 15) (name "Net-(J2-Pad14)")
      (node (ref R27) (pin 2))
      (node (ref J2) (pin 14)))
    (net (code 16) (name /TAPEOUT)
      (node (ref R24) (pin 1))
      (node (ref J2) (pin 16))
      (node (ref R25) (pin 1)))
    (net (code 17) (name "Net-(U10-Pad3)")
      (node (ref U11) (pin 2))
      (node (ref U10) (pin 3)))
    (net (code 18) (name BA*)
      (node (ref U6) (pin 1))
      (node (ref U6) (pin 15))
      (node (ref J5) (pin 11))
      (node (ref U5) (pin 15))
      (node (ref U11) (pin 12))
      (node (ref U5) (pin 1))
      (node (ref U12) (pin 12)))
    (net (code 19) (name BA)
      (node (ref U1) (pin 7))
      (node (ref U11) (pin 13)))
    (net (code 20) (name A14)
      (node (ref U10) (pin 10))
      (node (ref U11) (pin 1))
      (node (ref U1) (pin 24))
      (node (ref U9) (pin 23))
      (node (ref J4) (pin 16)))
    (net (code 21) (name A15)
      (node (ref U1) (pin 25))
      (node (ref U11) (pin 3))
      (node (ref U12) (pin 2))
      (node (ref J4) (pin 1)))
    (net (code 22) (name VMA)
      (node (ref U12) (pin 1))
      (node (ref U10) (pin 5))
      (node (ref U1) (pin 5)))
    (net (code 23) (name "Net-(U10-Pad4)")
      (node (ref U10) (pin 4))
      (node (ref U11) (pin 4)))
    (net (code 24) (name "Net-(U10-Pad2)")
      (node (ref U11) (pin 10))
      (node (ref U10) (pin 2)))
    (net (code 25) (name "Net-(J2-Pad9)")
      (node (ref R31) (pin 2))
      (node (ref J2) (pin 9)))
    (net (code 26) (name "Net-(J2-Pad8)")
      (node (ref U20) (pin 5))
      (node (ref J2) (pin 8))
      (node (ref U9) (pin 2)))
    (net (code 27) (name "Net-(J2-Pad6)")
      (node (ref J2) (pin 6))
      (node (ref U9) (pin 4))
      (node (ref U20) (pin 2)))
    (net (code 28) (name "Net-(J2-Pad5)")
      (node (ref J2) (pin 5))
      (node (ref U20) (pin 1))
      (node (ref U9) (pin 5)))
    (net (code 29) (name "Net-(J2-Pad4)")
      (node (ref U9) (pin 6))
      (node (ref J2) (pin 4)))
    (net (code 30) (name "Net-(J2-Pad3)")
      (node (ref J2) (pin 3))
      (node (ref U9) (pin 7)))
    (net (code 31) (name "Net-(J2-Pad2)")
      (node (ref J2) (pin 2))
      (node (ref U9) (pin 8)))
    (net (code 32) (name /RAMWR*)
      (node (ref U3) (pin 10))
      (node (ref U4) (pin 10))
      (node (ref U10) (pin 12)))
    (net (code 33) (name "Net-(Q2-Pad1)")
      (node (ref R15) (pin 1))
      (node (ref Q2) (pin 1)))
    (net (code 34) (name "Net-(C16-Pad2)")
      (node (ref R24) (pin 2))
      (node (ref C16) (pin 2)))
    (net (code 35) (name CASS.IN)
      (node (ref J3) (pin 1))
      (node (ref J3) (pin 13))
      (node (ref U9) (pin 17))
      (node (ref U21) (pin 8)))
    (net (code 36) (name CASS.OUT)
      (node (ref R14) (pin 1))
      (node (ref J3) (pin 10))
      (node (ref U9) (pin 10))
      (node (ref J3) (pin 8)))
    (net (code 37) (name VCO)
      (node (ref U24) (pin 3))
      (node (ref U20) (pin 9))
      (node (ref R22) (pin 2)))
    (net (code 38) (name "Net-(Q2-Pad2)")
      (node (ref Q2) (pin 2))
      (node (ref R13) (pin 1))
      (node (ref R14) (pin 2)))
    (net (code 39) (name "Net-(C14-Pad2)")
      (node (ref U24) (pin 7))
      (node (ref C14) (pin 2)))
    (net (code 40) (name "Net-(C13-Pad2)")
      (node (ref R20) (pin 1))
      (node (ref U24) (pin 6))
      (node (ref C13) (pin 2)))
    (net (code 41) (name "Net-(C13-Pad1)")
      (node (ref R15) (pin 2))
      (node (ref U24) (pin 5))
      (node (ref R16) (pin 1))
      (node (ref C13) (pin 1))
      (node (ref R17) (pin 2)))
    (net (code 42) (name "Net-(C16-Pad1)")
      (node (ref U24) (pin 4))
      (node (ref C16) (pin 1)))
    (net (code 43) (name "Net-(U21-Pad4)")
      (node (ref U21) (pin 4)))
    (net (code 44) (name "Net-(U22-Pad6)")
      (node (ref U22) (pin 6)))
    (net (code 45) (name "Net-(U21-Pad9)")
      (node (ref U21) (pin 9)))
    (net (code 46) (name "Net-(D5-Pad1)")
      (node (ref D5) (pin 1))
      (node (ref U23) (pin 6))
      (node (ref U21) (pin 12))
      (node (ref U22) (pin 5)))
    (net (code 47) (name "Net-(U21-Pad11)")
      (node (ref U21) (pin 11))
      (node (ref U22) (pin 1)))
    (net (code 48) (name "Net-(C15-Pad2)")
      (node (ref U22) (pin 10))
      (node (ref C15) (pin 2)))
    (net (code 49) (name "Net-(C15-Pad1)")
      (node (ref U22) (pin 11))
      (node (ref R21) (pin 2))
      (node (ref C15) (pin 1)))
    (net (code 50) (name "Net-(U21-Pad6)")
      (node (ref U21) (pin 6)))
    (net (code 51) (name "Net-(U21-Pad5)")
      (node (ref U21) (pin 5)))
    (net (code 52) (name "Net-(U21-Pad3)")
      (node (ref U21) (pin 3)))
    (net (code 53) (name "Net-(U21-Pad2)")
      (node (ref U21) (pin 2)))
    (net (code 54) (name "Net-(U21-Pad1)")
      (node (ref U21) (pin 1)))
    (net (code 55) (name "Net-(U22-Pad9)")
      (node (ref U22) (pin 9)))
    (net (code 56) (name "Net-(C36-Pad1)")
      (node (ref U23) (pin 3))
      (node (ref C36) (pin 1))
      (node (ref R32) (pin 2)))
    (net (code 57) (name "Net-(D5-Pad2)")
      (node (ref U23) (pin 2))
      (node (ref R28) (pin 2))
      (node (ref D5) (pin 2)))
    (net (code 58) (name "Net-(C6-Pad2)")
      (node (ref C6) (pin 2))
      (node (ref U19) (pin 14)))
    (net (code 59) (name "Net-(D1-Pad2)")
      (node (ref R4) (pin 1))
      (node (ref D1) (pin 2)))
    (net (code 60) (name "Net-(J1-Pad1)")
      (node (ref J1) (pin 1))
      (node (ref Q1) (pin 1))
      (node (ref R9) (pin 2)))
    (net (code 61) (name "Net-(D4-Pad2)")
      (node (ref R6) (pin 2))
      (node (ref D4) (pin 2)))
    (net (code 62) (name "Net-(C9-Pad2)")
      (node (ref C9) (pin 2))
      (node (ref R8) (pin 2))
      (node (ref R7) (pin 1))
      (node (ref R6) (pin 1))
      (node (ref Q1) (pin 2))
      (node (ref D2) (pin 2))
      (node (ref D3) (pin 2)))
    (net (code 63) (name "Net-(U6-Pad13)")
      (node (ref U6) (pin 13)))
    (net (code 64) (name "Net-(J2-Pad7)")
      (node (ref U9) (pin 3))
      (node (ref U20) (pin 4))
      (node (ref J2) (pin 7)))
    (net (code 65) (name "Net-(R21-Pad1)")
      (node (ref RV1) (pin 1))
      (node (ref RV2) (pin 1))
      (node (ref R21) (pin 1)))
    (net (code 66) (name A5)
      (node (ref U6) (pin 14))
      (node (ref U5) (pin 7))
      (node (ref U2) (pin 3))
      (node (ref U3) (pin 3))
      (node (ref U1) (pin 14))
      (node (ref J4) (pin 6))
      (node (ref U4) (pin 3)))
    (net (code 67) (name "Net-(U16-Pad11)")
      (node (ref U16) (pin 4))
      (node (ref U16) (pin 11))
      (node (ref U17) (pin 4)))
    (net (code 68) (name "Net-(U17-Pad12)")
      (node (ref U17) (pin 12))
      (node (ref U18) (pin 3)))
    (net (code 69) (name /H16)
      (node (ref U14) (pin 9))
      (node (ref U16) (pin 2))
      (node (ref U6) (pin 6)))
    (net (code 70) (name "Net-(U17-Pad8)")
      (node (ref U18) (pin 9))
      (node (ref U17) (pin 8)))
    (net (code 71) (name "Net-(U18-Pad11)")
      (node (ref U7) (pin 3))
      (node (ref U18) (pin 11)))
    (net (code 72) (name /VERT-EN)
      (node (ref U18) (pin 6))
      (node (ref U18) (pin 10))
      (node (ref U11) (pin 5)))
    (net (code 73) (name A11)
      (node (ref U1) (pin 20))
      (node (ref J4) (pin 3)))
    (net (code 74) (name A10)
      (node (ref U1) (pin 19))
      (node (ref J4) (pin 14)))
    (net (code 75) (name A9)
      (node (ref U1) (pin 18))
      (node (ref U2) (pin 22))
      (node (ref J4) (pin 4))
      (node (ref U5) (pin 3))
      (node (ref U4) (pin 16))
      (node (ref U3) (pin 16)))
    (net (code 76) (name A8)
      (node (ref J4) (pin 13))
      (node (ref U4) (pin 17))
      (node (ref U5) (pin 13))
      (node (ref U1) (pin 17))
      (node (ref U3) (pin 17))
      (node (ref U2) (pin 23)))
    (net (code 77) (name A7)
      (node (ref U4) (pin 1))
      (node (ref J4) (pin 5))
      (node (ref U2) (pin 1))
      (node (ref U1) (pin 16))
      (node (ref U5) (pin 5))
      (node (ref U3) (pin 1)))
    (net (code 78) (name A6)
      (node (ref U5) (pin 11))
      (node (ref U1) (pin 15))
      (node (ref J4) (pin 12))
      (node (ref U4) (pin 2))
      (node (ref U3) (pin 2))
      (node (ref U2) (pin 2)))
    (net (code 79) (name A4)
      (node (ref U1) (pin 13))
      (node (ref U4) (pin 15))
      (node (ref U3) (pin 15))
      (node (ref U9) (pin 24))
      (node (ref J4) (pin 11))
      (node (ref U2) (pin 4))
      (node (ref U5) (pin 9)))
    (net (code 80) (name A3)
      (node (ref J4) (pin 7))
      (node (ref U4) (pin 4))
      (node (ref U2) (pin 5))
      (node (ref U3) (pin 4))
      (node (ref U6) (pin 5))
      (node (ref U1) (pin 12)))
    (net (code 81) (name A2)
      (node (ref U2) (pin 6))
      (node (ref U1) (pin 11))
      (node (ref U4) (pin 5))
      (node (ref J4) (pin 10))
      (node (ref U6) (pin 11))
      (node (ref U3) (pin 5)))
    (net (code 82) (name A1)
      (node (ref U9) (pin 35))
      (node (ref U4) (pin 6))
      (node (ref U1) (pin 10))
      (node (ref U3) (pin 6))
      (node (ref U6) (pin 7))
      (node (ref J4) (pin 8))
      (node (ref U2) (pin 7)))
    (net (code 83) (name A0)
      (node (ref U4) (pin 7))
      (node (ref U6) (pin 9))
      (node (ref U3) (pin 7))
      (node (ref U1) (pin 9))
      (node (ref U9) (pin 36))
      (node (ref U2) (pin 8))
      (node (ref J4) (pin 9)))
    (net (code 84) (name A13)
      (node (ref J4) (pin 2))
      (node (ref U1) (pin 23)))
    (net (code 85) (name A12)
      (node (ref U1) (pin 22))
      (node (ref J4) (pin 15)))
    (net (code 86) (name "Net-(J3-Pad9)")
      (node (ref J3) (pin 9)))
    (net (code 87) (name D2)
      (node (ref U7) (pin 5))
      (node (ref U9) (pin 31))
      (node (ref U3) (pin 12))
      (node (ref U2) (pin 11))
      (node (ref U1) (pin 31))
      (node (ref J5) (pin 14)))
    (net (code 88) (name R/W*)
      (node (ref U11) (pin 11))
      (node (ref U10) (pin 11))
      (node (ref U9) (pin 21))
      (node (ref J5) (pin 6))
      (node (ref U1) (pin 34)))
    (net (code 89) (name D7)
      (node (ref U7) (pin 1))
      (node (ref U2) (pin 17))
      (node (ref J5) (pin 1))
      (node (ref U4) (pin 11))
      (node (ref U9) (pin 26))
      (node (ref U1) (pin 26)))
    (net (code 90) (name D6)
      (node (ref U2) (pin 16))
      (node (ref U7) (pin 15))
      (node (ref U1) (pin 27))
      (node (ref J5) (pin 16))
      (node (ref U4) (pin 12))
      (node (ref U9) (pin 27)))
    (net (code 91) (name D5)
      (node (ref U9) (pin 28))
      (node (ref U2) (pin 15))
      (node (ref U1) (pin 28))
      (node (ref U7) (pin 14))
      (node (ref U4) (pin 13))
      (node (ref J5) (pin 2)))
    (net (code 92) (name D4)
      (node (ref U9) (pin 29))
      (node (ref U2) (pin 14))
      (node (ref J5) (pin 15))
      (node (ref U1) (pin 29))
      (node (ref U7) (pin 13))
      (node (ref U4) (pin 14)))
    (net (code 93) (name D3)
      (node (ref U2) (pin 13))
      (node (ref U3) (pin 11))
      (node (ref U1) (pin 30))
      (node (ref U9) (pin 30))
      (node (ref U7) (pin 4))
      (node (ref J5) (pin 3)))
    (net (code 94) (name D1)
      (node (ref J5) (pin 4))
      (node (ref U2) (pin 10))
      (node (ref U3) (pin 13))
      (node (ref U1) (pin 32))
      (node (ref U7) (pin 6))
      (node (ref U9) (pin 32)))
    (net (code 95) (name D0)
      (node (ref J5) (pin 13))
      (node (ref U3) (pin 14))
      (node (ref U1) (pin 33))
      (node (ref U7) (pin 7))
      (node (ref U2) (pin 9))
      (node (ref U9) (pin 33)))
    (net (code 96) (name 02)
      (node (ref U10) (pin 1))
      (node (ref J5) (pin 7))
      (node (ref U8) (pin 7))
      (node (ref U9) (pin 25)))
    (net (code 97) (name "Net-(J3-Pad16)")
      (node (ref J3) (pin 16)))
    (net (code 98) (name "Net-(J3-Pad11)")
      (node (ref J3) (pin 11)))
    (net (code 99) (name RST*)
      (node (ref U1) (pin 40))
      (node (ref J5) (pin 9))
      (node (ref U8) (pin 14))
      (node (ref U9) (pin 34)))
    (net (code 100) (name VMA.A15)
      (node (ref J5) (pin 8))
      (node (ref U9) (pin 22))
      (node (ref U10) (pin 9))
      (node (ref U12) (pin 3)))
    (net (code 101) (name /PB5)
      (node (ref J3) (pin 3))
      (node (ref U9) (pin 15)))
    (net (code 102) (name /PB4)
      (node (ref J3) (pin 4))
      (node (ref U9) (pin 14)))
    (net (code 103) (name /PB3)
      (node (ref J3) (pin 5))
      (node (ref U9) (pin 13)))
    (net (code 104) (name /PB2)
      (node (ref U9) (pin 12))
      (node (ref J3) (pin 6)))
    (net (code 105) (name /PB1)
      (node (ref U9) (pin 11))
      (node (ref J3) (pin 7)))
    (net (code 106) (name IRQ*)
      (node (ref R12) (pin 2))
      (node (ref U1) (pin 4))
      (node (ref U9) (pin 37))
      (node (ref U9) (pin 38))
      (node (ref J5) (pin 10)))
    (net (code 107) (name "Net-(D4-Pad1)")
      (node (ref D4) (pin 1))
      (node (ref U18) (pin 8)))
    (net (code 108) (name "Net-(U17-Pad10)")
      (node (ref U17) (pin 10))
      (node (ref U18) (pin 4)))
    (net (code 109) (name "Net-(U19-Pad4)")
      (node (ref U19) (pin 4)))
    (net (code 110) (name "Net-(U19-Pad13)")
      (node (ref U19) (pin 13))
      (node (ref U7) (pin 9)))
    (net (code 111) (name "Net-(U7-Pad2)")
      (node (ref U7) (pin 2)))
    (net (code 112) (name "Net-(U7-Pad12)")
      (node (ref U7) (pin 12)))
    (net (code 113) (name "Net-(U17-Pad2)")
      (node (ref U17) (pin 2))
      (node (ref U7) (pin 10)))
    (net (code 114) (name "Net-(U14-Pad14)")
      (node (ref U14) (pin 14)))
    (net (code 115) (name "Net-(U16-Pad3-UB)")
      (node (ref U16) (pin 3-UB)))
    (net (code 116) (name "Net-(U16-Pad11-UB)")
      (node (ref U16) (pin 11-UB)))
    (net (code 117) (name "Net-(U14-Pad12)")
      (node (ref U14) (pin 12)))
    (net (code 118) (name /H4)
      (node (ref U19) (pin 1))
      (node (ref U15) (pin 8)))
    (net (code 119) (name "Net-(C6-Pad1)")
      (node (ref U19) (pin 15))
      (node (ref C6) (pin 1))
      (node (ref R2) (pin 2)))
    (net (code 120) (name /H32)
      (node (ref U6) (pin 12))
      (node (ref U14) (pin 8))
      (node (ref U17) (pin 3)))
    (net (code 121) (name /H8)
      (node (ref U6) (pin 10))
      (node (ref U14) (pin 1))
      (node (ref U15) (pin 11))
      (node (ref U16) (pin 5)))
    (net (code 122) (name /H64)
      (node (ref U16) (pin 3))
      (node (ref R3) (pin 1))
      (node (ref D1) (pin 1))
      (node (ref U14) (pin 11))
      (node (ref U16) (pin 1)))
    (net (code 123) (name "Net-(U13-Pad11)")
      (node (ref U13) (pin 11))
      (node (ref U17) (pin 6)))
    (net (code 124) (name "Net-(U16-Pad8)")
      (node (ref U16) (pin 8))
      (node (ref U17) (pin 5)))
    (net (code 125) (name "Net-(C7-Pad2)")
      (node (ref C7) (pin 2))
      (node (ref R3) (pin 2))
      (node (ref R4) (pin 2))
      (node (ref U17) (pin 9)))
    (net (code 126) (name /V64)
      (node (ref U13) (pin 12))
      (node (ref U17) (pin 13))
      (node (ref U16) (pin 13)))
    (net (code 127) (name /V32)
      (node (ref U18) (pin 2))
      (node (ref U13) (pin 13))
      (node (ref U17) (pin 11)))
    (net (code 128) (name /V16)
      (node (ref U18) (pin 13))
      (node (ref U5) (pin 4))
      (node (ref U13) (pin 4)))
    (net (code 129) (name /V4)
      (node (ref U13) (pin 3))
      (node (ref U5) (pin 6))
      (node (ref U16) (pin 10)))
    (net (code 130) (name /V1)
      (node (ref U13) (pin 6))
      (node (ref U6) (pin 4)))
    (net (code 131) (name "Net-(D2-Pad1)")
      (node (ref U13) (pin 10))
      (node (ref U16) (pin 6))
      (node (ref D2) (pin 1)))
    (net (code 132) (name "Net-(U13-Pad1)")
      (node (ref U13) (pin 1)))
    (net (code 133) (name "Net-(C8-Pad1)")
      (node (ref R5) (pin 1))
      (node (ref C8) (pin 1))
      (node (ref U19) (pin 7)))
    (net (code 134) (name "Net-(U18-Pad12)")
      (node (ref U19) (pin 10))
      (node (ref U18) (pin 12)))
    (net (code 135) (name "Net-(U13-Pad14)")
      (node (ref U13) (pin 14)))
    (net (code 136) (name /V2)
      (node (ref U16) (pin 9))
      (node (ref U13) (pin 5))
      (node (ref U5) (pin 10)))
    (net (code 137) (name /V8)
      (node (ref U16) (pin 12))
      (node (ref U18) (pin 1))
      (node (ref U5) (pin 12))
      (node (ref U13) (pin 2)))
    (net (code 138) (name "Net-(U13-Pad9)")
      (node (ref U13) (pin 9)))
    (net (code 139) (name "Net-(U13-Pad7)")
      (node (ref U13) (pin 7)))
    (net (code 140) (name "Net-(U13-Pad15)")
      (node (ref U13) (pin 15)))
    (net (code 141) (name "Net-(C11-Pad1)")
      (node (ref R10) (pin 1))
      (node (ref C11) (pin 1))
      (node (ref L2) (pin 2))
      (node (ref U8) (pin 1)))
    (net (code 142) (name "Net-(U8-Pad9)")
      (node (ref U8) (pin 9)))
    (net (code 143) (name "Net-(U8-Pad4)")
      (node (ref U8) (pin 4)))
    (net (code 144) (name "Net-(C11-Pad2)")
      (node (ref J8) (pin 1))
      (node (ref X1) (pin 2))
      (node (ref U8) (pin 2))
      (node (ref J8) (pin 2))
      (node (ref R10) (pin 2))
      (node (ref L2) (pin 1))
      (node (ref C11) (pin 2)))
    (net (code 145) (name "Net-(U1-Pad36)")
      (node (ref U1) (pin 36))
      (node (ref U1) (pin 37))
      (node (ref U8) (pin 13)))
    (net (code 146) (name EXT-RST)
      (node (ref J2) (pin 10))
      (node (ref U8) (pin 12))
      (node (ref C12) (pin 1)))
    (net (code 147) (name "Net-(U8-Pad11)")
      (node (ref U8) (pin 11)))
    (net (code 148) (name "Net-(U1-Pad3)")
      (node (ref U8) (pin 15))
      (node (ref U1) (pin 3)))
    (net (code 149) (name /H1)
      (node (ref U15) (pin 12))
      (node (ref U15) (pin 1)))
    (net (code 150) (name /H2)
      (node (ref U15) (pin 9)))
    (net (code 151) (name 2FO)
      (node (ref U15) (pin 14))
      (node (ref U17) (pin 1))
      (node (ref U8) (pin 5)))
    (net (code 152) (name HALT*)
      (node (ref U11) (pin 6))
      (node (ref U1) (pin 2)))
    (net (code 153) (name "Net-(U20-Pad3-UB)")
      (node (ref U20) (pin 3-UB)))
    (net (code 154) (name "Net-(U20-Pad11-UB)")
      (node (ref U20) (pin 11-UB)))
    (net (code 155) (name RTC)
      (node (ref U9) (pin 18))
      (node (ref J3) (pin 14))
      (node (ref U19) (pin 5)))
    (net (code 156) (name "Net-(U20-Pad6)")
      (node (ref U9) (pin 40))
      (node (ref U20) (pin 6)))
    (net (code 157) (name "Net-(U20-Pad3)")
      (node (ref U20) (pin 3)))
    (net (code 158) (name "Net-(U20-Pad11)")
      (node (ref U20) (pin 11)))
    (net (code 159) (name /PB6)
      (node (ref U20) (pin 13))
      (node (ref U20) (pin 12))
      (node (ref J3) (pin 12))
      (node (ref J3) (pin 2))
      (node (ref U9) (pin 16)))
    (net (code 160) (name "Net-(U23-Pad5)")
      (node (ref U23) (pin 5)))
    (net (code 161) (name "Net-(U23-Pad1)")
      (node (ref U23) (pin 1)))
    (net (code 162) (name "Net-(J2-Pad1)")
      (node (ref U9) (pin 9))
      (node (ref J2) (pin 1)))
    (net (code 163) (name DMA.ENAB)
      (node (ref U9) (pin 19))
      (node (ref J3) (pin 15))
      (node (ref U18) (pin 5))
      (node (ref R18) (pin 1))
      (node (ref U20) (pin 10)))
    (net (code 164) (name "Net-(R23-Pad1)")
      (node (ref U12) (pin 8))
      (node (ref U9) (pin 39))
      (node (ref R23) (pin 1)))
    (net (code 165) (name "Net-(R23-Pad2)")
      (node (ref R26) (pin 1))
      (node (ref R23) (pin 2))
      (node (ref U12) (pin 10))
      (node (ref U12) (pin 9)))
    (net (code 166) (name /VSYNC*)
      (node (ref U19) (pin 12))
      (node (ref D3) (pin 1)))))